Legend and Statistics

0 AC crashes into landing zone near E1 taxiway

1 AC stalls since

2 CRW unable to recover stall

1.1.2.1.1 EPR increased from 1.04 to > 1.6

1.1.2.1.1.1 THR levers moved forward

1.1.2.1.1.2 Alpha Floor Function activated

1.1.2 AC climbing steeply

1.1.2.1 high engine thrust

1.1.2.2 F/O releases control wheel

2.2 AC systems in unusual modes

2.2.1 complex control situation at stall 2.2.1.1

trying to transit GO-AROUND -> LAND

2.3 time and altitude for recovery operations short to insufficient

2.3.1 nose-up attitude is 43.8 degrees

2.3.2 altitude is 1,730ft

2.3.3 AS is less than 50kts

1.1 AOA becomes too large

2.1 CRW doesn’t take appropriate action to recover stall